**TEATRO TATRO / Technical Rider**

**LITTLE RED RIDING HOOD**

* Requested area for placement of a tent – flat ground of 10 x 20m, it counts with guy lines and base (if there is grass, please mow the spot under the tent)

Way of anchoring: on the grass – pounding stakes into the ground (to the depth of 30 cm)

* Road access for a truck and actors‘ cars
* Parking for a truck and actors‘ cars
* Electric connection: 220V
* 2 helpers to carry out setup and takedown of the tent – on the day of the performance at the time agreed in advance with the production

* Service of an organizer during the performance
* Overnight tent guarding in case of multi-day performing
* 16 pcs of benches for spectators
* Mobile toilet for actors in proximity to the tent
* Sufficient amount of drinking water – still mineral water for 10 persons during setup / takedown of the tent and during the performance
* Auditorium capacity: 70 spectators

***CONTACT***

Production: Jana Suraová, +421 905 265 947, [mana@mana.sk](mailto:mana@mana.sk)